{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Arkusz1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Arkusz1","index":0,"n_rows":18,"n_cols":7,"rows_kept":18,"cut":false,"hidden":false,"merged":[[17,1,24,6]],"flags":["formulas_cached_only"]}
["Produkt","Składnik","Ilość","JM","Etap","Technologia","Grupa produkcyjna"]
[null,"Produkt A",1,"szt","Import","Technologia Produktu A","Grupa Produktu A"]
["Produkt A","Półprodukt A",1,"szt","Montaż","Technologia Półproduktu A","Grupa Półproduktu A"]
["Produkt A","Półprodukt B",2,"szt","Montaż","Technologia Półproduktu B","Grupa Półproduktu B"]
["Produkt A","Składnik A1",2.3,"m2","Spawanie"]
["Produkt A","Składnik A2",1.75,"kg","Spawanie"]
["Półprodukt A","Składnik Z3",2,"mb","Cięcie"]
["Półprodukt A","Składnik Z4",4,"mb","Cięcie"]
["Półprodukt A","Składnik Z5",3,"szt","Montaż"]
["Półprodukt A","Składnik Z6",12,"szt","Montaż"]
["Półprodukt B","Składnik C5",6,"szt","Montaż"]
["Półprodukt B","Składnik c6",10,"szt","Montaż"]
[]
[]
[]
[]
[]
[null,"Produkt A należący do grupy produkcyjnej ‘Grupa Produktu A’ jest wykonywany w technologii ‘Technologia Produktu A’, składa się z półproduktów Półprodukt A i Półprodukt B oraz z dwóch składników. Technologia Produktu A jest parta na dwóch etapach – Montaż i Spawanie. Półprodukt A należy do grupy ‘Grupa Półproduktu A’, wykonywany jest w technologii ‘Technologia Półproduktu A’ składającej się z dwóch etapów – Cięcie i Montaż. Na etapie Cięcie wykorzystywane będą składniki – Składnik Z3 i Składnik Z4, na etapie Montaż: Składnik Z5 i Składnik Z6…"]